(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 98)
    (zones 0)
    (modules 16)
    (nets 14)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 0.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 +15V)
  (net 2 GNDA)
  (net 3 -15V)
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J2-Pad2)")
  (net 6 /inB-)
  (net 7 /inA-)
  (net 8 "Net-(RA1-Pad1)")
  (net 9 /outA)
  (net 10 "Net-(RA3-Pad2)")
  (net 11 "Net-(RB1-Pad1)")
  (net 12 /outB)
  (net 13 "Net-(RB3-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /inA-)
    (add_net /inB-)
    (add_net /outA)
    (add_net /outB)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(RA1-Pad1)")
    (add_net "Net-(RA3-Pad2)")
    (add_net "Net-(RB1-Pad1)")
    (add_net "Net-(RB3-Pad2)")
  )

  (net_class power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net -15V)
    (add_net GNDA)
  )

  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5C548E98)
    (at 101.6 38.1)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5C54CA7D)
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM4562 (at 3.81 9.95) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 8.89) (end 0.635 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 8.89) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 8.95) (end 6.46 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 8.95) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 9.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 9.15) (end 8.7 9.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 9.15) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /outA))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(RB3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(RA1-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(RB1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(RA3-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /outB))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -15V))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PCIexpress_1x_letters (layer F.Cu) (tedit 5C5476B0) (tstamp 5C54794C)
    (at 96.52 66.04)
    (descr "PCIexpress Bus Edge Connector")
    (tags "PCIexpress Bus Edge Connector")
    (path /5C5482AB)
    (attr virtual)
    (fp_text reference J3 (at 5.05 -3.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_02x18_Row_Letter_First (at 16.48 -3.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 19.95 4.05) (end -0.95 4.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 19.95 4.05) (end 19.95 -5.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -5.45) (end -0.95 4.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -5.45) (end 19.95 -5.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start 19.7 -2) (end 19.7 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.4 -2) (end 12.4 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.4 3.8) (end 19.7 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 19.7 -2) (end 12.4 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 3.8) (end -0.7 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 3.8) (end -0.7 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -2) (end 10.6 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -2) (end 10.6 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.4 -5.2) (end 12.4 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -5.2) (end 12.4 -5.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -2) (end 10.6 -5.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 9.5 0.662) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad "" connect oval (at 1 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 19 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 18 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 13 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 10 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 17 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 14 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 2 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 16 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 15 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 9 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 8 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 7 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 6 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 5 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 4 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 3 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect circle (at 1 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 17 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 16 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 15 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 14 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 13 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 0 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 10 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 9 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 8 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 7 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 6 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 5 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 4 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 3 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 2 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad 13a connect rect (at 14 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 12a connect rect (at 13 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 18a connect rect (at 19 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 17a connect rect (at 18 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 16a connect rect (at 17 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 15a connect rect (at 16 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 14a connect rect (at 15 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 11a connect rect (at 10 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 10a connect rect (at 9 0.5) (size 0.65 4.6) (layers B.Cu B.Mask))
    (pad 9a connect rect (at 8 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 1 +15V))
    (pad 8a connect rect (at 7 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 1 +15V))
    (pad 7a connect rect (at 6 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 1 +15V))
    (pad 6a connect rect (at 5 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 5a connect rect (at 4 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 4a connect rect (at 3 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 3a connect rect (at 2 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 3 -15V))
    (pad 2a connect rect (at 1 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 3 -15V))
    (pad 1a connect rect (at 0 0) (size 0.65 3.6) (layers B.Cu B.Mask)
      (net 3 -15V))
    (pad 13b connect rect (at 14 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 12b connect rect (at 13 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 18b connect rect (at 19 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 17b connect rect (at 18 0) (size 0.65 3.6) (layers F.Cu F.Mask))
    (pad 16b connect rect (at 17 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 15b connect rect (at 16 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 14b connect rect (at 15 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 11b connect rect (at 10 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 10b connect rect (at 9 0.5) (size 0.65 4.6) (layers F.Cu F.Mask))
    (pad 9b connect rect (at 8 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 1 +15V))
    (pad 8b connect rect (at 7 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 1 +15V))
    (pad 7b connect rect (at 6 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 1 +15V))
    (pad 6b connect rect (at 5 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 5b connect rect (at 4 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 4b connect rect (at 3 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 3b connect rect (at 2 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 3 -15V))
    (pad 2b connect rect (at 1 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 3 -15V))
    (pad 1b connect rect (at 0 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 3 -15V))
    (pad "" connect circle (at 19 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5C5490AB)
    (at 109.26 35.56 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5C54CB2B)
    (fp_text reference CU1+1 (at 1.25 -2.05 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +15V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5C54904A)
    (at 104.1 48.26 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5C54CB3A)
    (fp_text reference CU1-1 (at 1.25 -2.05 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -15V))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C549AAD)
    (at 96.52 53.34 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CA8C)
    (fp_text reference RA2 (at 3.81 -1.92 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(RA1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C5492E5)
    (at 91.44 43.18)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAA4)
    (fp_text reference RA3 (at 3.81 -1.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(RA3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /inA-))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C54819D)
    (at 93.98 45.72 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAB9)
    (fp_text reference RA4 (at 3.81 -1.92 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10 (at 3.81 1.92 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548D58)
    (at 99.06 45.72 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAAC)
    (fp_text reference RA5 (at 3.81 -1.92 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(RA3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C5481CB)
    (at 119.38 40.64 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CB19)
    (fp_text reference RB1 (at 3.81 -1.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(RB1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 /outB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548E51)
    (at 114.3 55.88 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAD8)
    (fp_text reference RB2 (at 3.81 -1.92 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(RB1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548E0F)
    (at 119.38 45.72 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAE4)
    (fp_text reference RB3 (at 3.81 -1.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(RB3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 /inB-))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548D9A)
    (at 116.84 48.26 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAF8)
    (fp_text reference RB4 (at 3.81 -1.92 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10 (at 3.81 1.92 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548D16)
    (at 111.76 50.8 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAEC)
    (fp_text reference RB5 (at 3.81 -1.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(RB3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66) (tstamp 5C548DD7)
    (at 118.76 43.18 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /5C54CB0B)
    (attr virtual)
    (fp_text reference J1 (at 0 1.8 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Jumper (at 0 -1.9 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.7 1) (end 0.7 1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 0.3) (end 1.4 -0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.7 -1) (end -0.7 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.3) (end -1.4 0.3) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 0.3) (end -0.7 1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 -0.3) (end -1.4 -0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 -0.3) (end 0.7 -1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 0.3) (end 1.4 0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 4 "Net-(J1-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 6 /inB-) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66) (tstamp 5C549344)
    (at 92.06 40.64)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /5C54CACC)
    (attr virtual)
    (fp_text reference J2 (at 0 1.8) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Jumper (at 0 -1.9) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_arc (start 0.7 0.3) (end 1.4 0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 -0.3) (end 0.7 -1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 -0.3) (end -1.4 -0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 0.3) (end -0.7 1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.3) (end -1.4 0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.7 -1) (end -0.7 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 0.3) (end 1.4 -0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 1) (end 0.7 1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 7 /inA-) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 5 "Net-(J2-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C549444)
    (at 91.44 38.1)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CA95)
    (fp_text reference RA1 (at 3.81 -1.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(RA1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 /outA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (segment (start 109.22 35.6) (end 109.26 35.56) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 109.22 38.1) (end 109.22 35.6) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 98.52 66.54) (end 98.52 62.325) (width 0.5) (layer B.Cu) (net 3) (status 10))
  (segment (start 98.52 62.325) (end 98.425 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 96.52 62.23) (end 96.52 66.04) (width 0.5) (layer B.Cu) (net 3) (status 20))
  (segment (start 97.52 62.595) (end 97.155 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 97.52 66.54) (end 97.52 62.595) (width 0.5) (layer B.Cu) (net 3) (status 10))
  (segment (start 97.155 62.23) (end 96.52 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 98.425 62.23) (end 97.155 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 96.52 66.54) (end 96.52 62.23) (width 0.5) (layer F.Cu) (net 3) (status 10))
  (segment (start 98.52 62.325) (end 98.52 66.54) (width 0.5) (layer F.Cu) (net 3) (status 20))
  (segment (start 98.425 62.23) (end 98.52 62.325) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.52 62.595) (end 97.52 66.54) (width 0.5) (layer F.Cu) (net 3) (status 20))
  (segment (start 97.155 62.23) (end 97.52 62.595) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.79 62.23) (end 97.155 62.23) (width 0.5) (layer F.Cu) (net 3))
  (via (at 97.79 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 3) (tstamp 5C54983B))
  (segment (start 96.52 62.23) (end 97.79 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.79 62.23) (end 98.425 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 106.76 35.56) (end 105.49 36.83) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 105.49 46.87) (end 104.1 48.26) (width 1) (layer B.Cu) (net 2) (status 20))
  (segment (start 105.49 36.83) (end 105.49 46.87) (width 1) (layer B.Cu) (net 2))
  (segment (start 104.1 48.26) (end 104.1 52.11) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 104.1 52.11) (end 102.87 53.34) (width 1) (layer B.Cu) (net 2))
  (segment (start 99.52 66.54) (end 99.52 62.405) (width 0.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 101.52 62.785) (end 101.52 66.54) (width 0.5) (layer B.Cu) (net 2) (status 20))
  (segment (start 100.965 62.23) (end 101.52 62.785) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.52 62.675) (end 100.965 62.23) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.52 66.54) (end 100.52 62.675) (width 0.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 99.695 62.23) (end 100.33 62.23) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.33 62.23) (end 100.965 62.23) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 99.52 63.04) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.52 66.54) (end 99.52 63.04) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 100.52 62.42) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 100.52 66.54) (end 100.52 62.42) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 101.52 63.42) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 101.52 66.54) (end 101.52 63.42) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 99.52 62.405) (end 99.695 62.23) (width 0.5) (layer B.Cu) (net 2))
  (via (at 100.33 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 100.33 62.23) (end 100.33 53.34) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.33 53.34) (end 99.06 53.34) (width 1) (layer B.Cu) (net 2) (status 20))
  (segment (start 102.87 53.34) (end 100.33 53.34) (width 1) (layer B.Cu) (net 2))
  (segment (start 101.6 45.72) (end 101.6 48.26) (width 1) (layer B.Cu) (net 3) (status 30))
  (segment (start 102.52 66.54) (end 102.52 62.58) (width 0.5) (layer B.Cu) (net 1) (status 10))
  (segment (start 102.52 62.58) (end 102.87 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 104.52 62.61) (end 104.52 66.54) (width 0.5) (layer B.Cu) (net 1) (status 20))
  (segment (start 104.14 62.23) (end 104.52 62.61) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 103.52 66.54) (end 103.52 62.245) (width 0.5) (layer B.Cu) (net 1) (status 10))
  (segment (start 103.505 62.23) (end 104.14 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 102.87 62.23) (end 103.505 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 103.52 62.245) (end 103.505 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 102.52 63.215) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 102.52 66.54) (end 102.52 63.215) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 103.52 62.245) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 103.52 66.54) (end 103.52 62.245) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 104.52 63.245) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 104.52 66.54) (end 104.52 63.245) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (via (at 103.505 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 1))
  (segment (start 109.22 38.1) (end 107.95 38.1) (width 1) (layer F.Cu) (net 1))
  (segment (start 107.95 38.1) (end 106.68 39.37) (width 1) (layer F.Cu) (net 1))
  (segment (start 106.68 59.055) (end 103.505 62.23) (width 1) (layer F.Cu) (net 1))
  (segment (start 106.68 39.37) (end 106.68 59.055) (width 1) (layer F.Cu) (net 1))
  (segment (start 93.98 53.34) (end 93.98 52.07) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 95.25 50.8) (end 97.79 50.8) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 93.98 52.07) (end 95.25 50.8) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 99.06 52.07) (end 99.06 53.34) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 97.79 50.8) (end 99.06 52.07) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 116.84 55.88) (end 116.84 54.61) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 116.84 54.61) (end 115.57 53.34) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 115.57 53.34) (end 102.87 53.34) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 101.6 50.8) (end 101.6 48.26) (width 1) (layer F.Cu) (net 3) (status 20))
  (segment (start 101.6 50.8) (end 101.6 54.61) (width 1) (layer F.Cu) (net 3))
  (segment (start 97.79 58.42) (end 97.79 62.23) (width 1) (layer F.Cu) (net 3))
  (segment (start 101.6 54.61) (end 97.79 58.42) (width 1) (layer F.Cu) (net 3))
  (segment (start 118.11 43.18) (end 116.84 44.45) (width 1) (layer B.Cu) (net 4))
  (segment (start 116.84 44.45) (end 116.84 48.26) (width 1) (layer B.Cu) (net 4))
  (segment (start 92.71 40.64) (end 93.98 41.91) (width 1) (layer B.Cu) (net 5))
  (segment (start 93.98 45.72) (end 93.98 41.91) (width 1) (layer B.Cu) (net 5))
  (segment (start 119.41 45.69) (end 119.38 45.72) (width 1) (layer F.Cu) (net 6) (status 30))
  (segment (start 119.41 45.69) (end 119.38 45.72) (width 1) (layer B.Cu) (net 6))
  (segment (start 119.41 43.18) (end 119.41 45.69) (width 1) (layer B.Cu) (net 6))
  (segment (start 91.41 43.15) (end 91.44 43.18) (width 1) (layer B.Cu) (net 7))
  (segment (start 91.41 40.64) (end 91.41 43.15) (width 1) (layer B.Cu) (net 7))
  (segment (start 99.06 40.64) (end 96.52 40.64) (width 1) (layer B.Cu) (net 8) (status 10))
  (segment (start 96.52 40.64) (end 93.98 38.1) (width 1) (layer B.Cu) (net 8))
  (segment (start 93.98 38.1) (end 91.44 38.1) (width 1) (layer B.Cu) (net 8) (status 20))
  (segment (start 101.6 40.64) (end 99.06 40.64) (width 1) (layer B.Cu) (net 8) (status 30))
  (segment (start 96.52 45.72) (end 96.52 40.64) (width 1) (layer B.Cu) (net 8))
  (segment (start 99.06 38.1) (end 101.6 38.1) (width 1) (layer B.Cu) (net 9) (status 30))
  (segment (start 101.6 43.18) (end 99.06 43.18) (width 1) (layer B.Cu) (net 10) (status 30))
  (segment (start 99.06 43.18) (end 99.06 45.72) (width 1) (layer B.Cu) (net 10) (status 30))
  (segment (start 109.22 43.18) (end 111.76 43.18) (width 1) (layer B.Cu) (net 11) (status 30))
  (segment (start 119.38 40.64) (end 116.84 40.64) (width 1) (layer B.Cu) (net 11) (status 10))
  (segment (start 114.3 43.18) (end 111.76 43.18) (width 1) (layer B.Cu) (net 11) (status 20))
  (segment (start 116.84 40.64) (end 114.3 43.18) (width 1) (layer B.Cu) (net 11))
  (segment (start 114.3 48.26) (end 114.3 43.18) (width 1) (layer B.Cu) (net 11))
  (segment (start 111.76 40.64) (end 109.22 40.64) (width 1) (layer B.Cu) (net 12) (status 30))
  (segment (start 111.76 45.72) (end 109.22 45.72) (width 1) (layer B.Cu) (net 13) (status 30))
  (segment (start 111.76 45.72) (end 111.76 50.8) (width 1) (layer B.Cu) (net 13))

)
