config defaults
        option syn_flood        1
        option input            ACCEPT
        option output           ACCEPT
        option forward          REJECT

config zone
        option name             lan
        option input    ACCEPT
        option output   ACCEPT
        option forward  REJECT

config zone
        option name             wan
        option input    REJECT
        option output   ACCEPT
        option forward  REJECT
        option masq             1

config forwarding
        option src      lan
        option dest     wan

## Enable this option if you encounter any MTU problems
## e.g. some websites work, others do not, submitting
## forms causes problems, ...
#       option mtu_fix  1


### EXAMPLE CONFIG SECTIONS
# do not allow a specific ip to access wan
#config rule
#       option src              lan
#       option src_ip   192.168.45.2
#       option dest             wan
#       option proto    tcp
#       option target   REJECT

# block a specific mac on wan
#config rule
#       option dest             wan
#       option src_mac  00:11:22:33:44:66
#       option target   REJECT

# block incoming ICMP traffic on a zone
#config rule
#       option src              lan
#       option proto    ICMP
#       option target   DROP

# port redirect port coming in on wan to lan
#config redirect
#       option src                      wan
#       option src_dport        80
#       option dest                     lan
#       option dest_ip          192.168.16.235
#       option dest_port        80
#       option proto            tcp

# include a file with users custom iptables rules
config include
       option path /etc/firewall.user


### FULL CONFIG SECTIONS
#config rule
#       option src              lan
#       option src              lan
#       option src_ip   192.168.45.2
#       option src_mac  00:11:22:33:44:55
#       option src_port 80
#       option dest             wan
#       option dest_ip  194.25.2.129
#       option dest_port        120
#       option proto    tcp
#       option target   REJECT

#config redirect
#       option src              lan
#       option src_ip   192.168.45.2
#       option src_mac  00:11:22:33:44:55
#       option src_port         1024
#       option src_dport        80
#       option dest_ip  194.25.2.129
#       option dest_port        120
#       option proto    tcp

