#!/bin/sh /etc/rc.common

START=70
EXTRA_COMMANDS=clear_leases
LIMIT_DOWN=0
LIMIT_DOWN_BURST=0
LIMIT_UP=0

IPT_REPLAY=/var/run/luci_splash.iptlog
LOCK=/var/run/luci_splash.lock

include /lib/network
scan_interfaces
config_load luci_splash

silent() {
	"$@" 2>/dev/null
}

ipt_log() {
	iptables -I "$@"
	echo iptables -D "$@" >> $IPT_REPLAY
}

iface_add() {
	local cfg="$1"
	
	config_get zone "$cfg" zone
	[ -n "$zone" ] || return 0
	
	config_get net "$cfg" network
	[ -n "$net" ] || return 0

	config_get ifname "$net" ifname
	[ -n "$ifname" ] || return 0
	
	config_get ipaddr "$net" ipaddr
	[ -n "$ipaddr" ] || return 0
	
	config_get netmask "$net" netmask
	[ -n "$netmask" ] || return 0
	
	config_get parentiface "$net" interface
	[ -n "$parentiface" ] && {
		config_get parentproto   "$parentiface" proto
		config_get parentipaddr  "$parentiface" ipaddr
		config_get parentnetmask "$parentiface" netmask
	}
	
	eval "$(ipcalc.sh $ipaddr $netmask)"

	### Add interface specific chain entry rules
	ipt_log "zone_${zone}_prerouting" -i "${ifname%:*}" -s "$NETWORK/$PREFIX" -j luci_splash_prerouting -t nat
	ipt_log "zone_${zone}_forward"    -i "${ifname%:*}" -s "$NETWORK/$PREFIX" -j luci_splash_forwarding -t filter

	### Allow traffic to the same subnet
	iptables -t nat    -I luci_splash_prerouting -d "$ipaddr/${netmask:-32}" -j RETURN
	iptables -t filter -I luci_splash_forwarding -d "$ipaddr/${netmask:-32}" -j RETURN

	### Allow traffic to the mesh subnet
	[ "$parentproto" = "static" -a -n "$parentipaddr" ] && {
		iptables -t nat    -I luci_splash_prerouting -d "$parentipaddr/${parentnetmask:-32}" -j RETURN
		iptables -t filter -I luci_splash_forwarding -d "$parentipaddr/${parentnetmask:-32}" -j RETURN
	}

	qos_iface_add "$ifname"
}

iface_del() {
	config_get zone "$1" zone                                                                
	[ -n "$zone" ] || return 0

	config_get net "$1" network
	[ -n "$net" ] || return 0

	config_get ifname "$net" ifname
	[ -n "$ifname" ] || return 0

	# Clear interface specific rules
	[ -s $IPT_REPLAY ] && {
		grep -- "-i ${ifname%:*}" $IPT_REPLAY | while read ln; do silent $ln; done
		sed -ie "/-i ${ifname%:*}/d" $IPT_REPLAY
	}

	qos_iface_del "$ifname"
}

mac_add() {
	config_get mac "$1" mac
	append MACS "$mac"
}

subnet_add() {
	local cfg="$1"
	
	config_get ipaddr  "$cfg" ipaddr
	config_get netmask "$cfg" netmask
	
	[ -n "$ipaddr" ] && {
		iptables -t nat    -I luci_splash_prerouting -d "$ipaddr/${netmask:-32}" -j RETURN
		iptables -t filter -I luci_splash_forwarding -d "$ipaddr/${netmask:-32}" -j RETURN
	}
}

qos_iface_add() {
	local iface="$1"

	# 77 -> download root qdisc
	# 78 -> upload root qdisc
	# 79 -> fwmark: client->inet
	# 80 -> fwmark: inet->client

	silent tc qdisc del dev "$iface" root handle 77:

	if [ "$LIMIT_UP" -gt 0 -a "$LIMIT_DOWN" -gt 0 ]; then
		tc qdisc add dev "$iface" root handle 77: htb

		# assume maximum rate of 20.000 kilobit for wlan
		tc class add dev "$iface" parent 77: classid 77:1 htb rate 20000kbit

		# set download limit and burst
		tc class add dev "$iface" parent 77:1 classid 77:10 htb \
			rate ${LIMIT_DOWN}kbit ceil ${LIMIT_DOWN_BURST}kbit prio 2

		tc qdisc add dev "$iface" parent 77:10 handle 78: sfq perturb 10

		# adding ingress can result in "File exists" if qos-scripts are active
		silent tc qdisc add dev "$iface" ingress

		# set client download speed
		tc filter add dev "$iface" parent 77: protocol ip prio 2 \
			handle 80 fw flowid 77:10

		# set client upload speed
		tc filter add dev "$iface" parent ffff: protocol ip prio 1 \
			handle 79 fw police rate ${LIMIT_UP}kbit mtu 6k burst 6k drop
	fi	
}

qos_iface_del() {
	local iface="$1"

	silent tc qdisc del dev "$iface" root handle 77:
	silent tc qdisc del dev "$iface" root handle 78:
	silent tc filter del dev "$iface" parent ffff: protocol ip prio 1 handle 79 fw
}

boot() {
	### Setup splash-relay
	uci get lucid.splashr 2>/dev/null || {
uci batch <<EOF
	set lucid.splashr=daemon
	set lucid.splashr.slave=httpd
	add_list lucid.splashr.address=8082
	add_list lucid.splashr.publisher=splashredir
	set lucid.splashr.enabled=1

	set lucid.splashredir=Redirector
	set lucid.splashredir.name=Splashd
	set lucid.splashredir.virtual='/'
	set lucid.splashredir.physical=':80/luci/splash'

	commit lucid
EOF
	}

	### We are started by the firewall include
	exit 0
}

start() {
	lock -w $LOCK && lock $LOCK

	### Find QoS limits
	config_get LIMIT_UP general limit_up
	config_get LIMIT_DOWN general limit_down
	config_get LIMIT_DOWN_BURST general limit_down_burst

	LIMIT_UP="$((8*${LIMIT_UP:-0}))"
	LIMIT_DOWN="$((8*${LIMIT_DOWN:-0}))"
	LIMIT_DOWN_BURST="${LIMIT_DOWN_BURST:+$((8*$LIMIT_DOWN_BURST))}"
	LIMIT_DOWN_BURST="${LIMIT_DOWN_BURST:-$(($LIMIT_DOWN / 5 * 6))}"

	### Load required modules
	[ "$LIMIT_UP" -gt 0 -a "$LIMIT_DOWN" -gt 0 ] && {
		silent insmod cls_fw
		silent insmod cls_u32
		silent insmod sch_htb
		silent insmod sch_sfq
		silent insmod sch_ingress
	}

	### Create subchains
	iptables -t nat    -N luci_splash_prerouting
	iptables -t nat    -N luci_splash_leases
	iptables -t filter -N luci_splash_forwarding
	iptables -t filter -N luci_splash_filter

	### Clear iptables replay log
	[ -s $IPT_REPLAY ] && . $IPT_REPLAY
	echo -n > $IPT_REPLAY

	### Build the main and portal rule
	config_foreach iface_add iface
	config_foreach subnet_add subnet

	### Add interface independant prerouting rules
	iptables -t nat -A luci_splash_prerouting -j luci_splash_leases
	iptables -t nat -A luci_splash_leases -p udp --dport 53 -j REDIRECT --to-ports 53
	iptables -t nat -A luci_splash_leases -p tcp --dport 80 -j REDIRECT --to-ports 8082

	### Add interface independant forwarding rules
	iptables -t filter -A luci_splash_forwarding -j luci_splash_filter
	iptables -t filter -A luci_splash_filter -p tcp -j REJECT --reject-with tcp-reset
	iptables -t filter -A luci_splash_filter -j REJECT --reject-with icmp-net-prohibited

	### Add QoS chain
	[ "$LIMIT_UP" -gt 0 -a "$LIMIT_DOWN" -gt 0 ] && {
		iptables -t mangle -N luci_splash_mark_out
		iptables -t mangle -N luci_splash_mark_in
		iptables -t mangle -I PREROUTING  -j luci_splash_mark_out
		iptables -t mangle -I POSTROUTING -j luci_splash_mark_in
	}

	### Find active mac addresses
	MACS=""
	config_foreach mac_add lease
	config_foreach mac_add blacklist
	config_foreach mac_add whitelist

	### Add crontab entry
	test -f /etc/crontabs/root || touch /etc/crontabs/root
	grep -q luci-splash /etc/crontabs/root || {
		echo '*/5 * * * * 	/usr/sbin/luci-splash sync' >> /etc/crontabs/root
	}

	lock -u $LOCK

	### Populate iptables
	[ -n "$MACS" ] && luci-splash add-rules $MACS
}

stop() {
	lock -w $LOCK && lock $LOCK

	### Clear interface rules
	config_foreach iface_del iface

	silent iptables -t mangle -D PREROUTING  -j luci_splash_mark_out
	silent iptables -t mangle -D POSTROUTING -j luci_splash_mark_in
        
	### Clear subchains
	silent iptables -t nat    -F luci_splash_prerouting
	silent iptables -t nat    -F luci_splash_leases
	silent iptables -t filter -F luci_splash_forwarding
	silent iptables -t filter -F luci_splash_filter
	silent iptables -t mangle -F luci_splash_mark_out
	silent iptables -t mangle -F luci_splash_mark_in
	
	### Delete subchains
	silent iptables -t nat    -X luci_splash_prerouting
	silent iptables -t nat    -X luci_splash_leases
	silent iptables -t filter -X luci_splash_forwarding
	silent iptables -t filter -X luci_splash_filter
	silent iptables -t mangle -X luci_splash_mark_out
	silent iptables -t mangle -X luci_splash_mark_in
	
	sed -ie '/\/usr\/sbin\/luci-splash sync/d' /var/spool/cron/crontabs/root

	lock -u $LOCK
}

clear_leases() {
	### Find active mac addresses
	MACS=""
	config_foreach mac_add lease

	### Clear leases
	[ -n "$MACS" ] && luci-splash remove $MACS
}

