(module PCIexpress_1x_connector (layer F.Cu) (tedit 5D08AB2A)
  (fp_text reference REF** (at -14.28 5.355) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PCIexpress_1x_connector (at -12.495 -10.71) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3 5.5) (end -3 5) (layer F.SilkS) (width 0.15))
  (fp_line (start 22 5.5) (end -3 5.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 22 5) (end 22 5.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 5) (end -3 -2.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 22 5.3) (end -3 5.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 22 -2.8) (end 22 5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -2.8) (end 22 -2.8) (layer F.SilkS) (width 0.15))
  (pad "" thru_hole circle (at 20.65 1.25) (size 2.35 2.35) (drill 2.35) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 11.65 1.25) (size 2.35 2.35) (drill 2.35) (layers *.Cu *.Mask))
  (pad 18b thru_hole circle (at 19 4.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 17b thru_hole circle (at 18 2.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 16b thru_hole circle (at 17 4.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 15b thru_hole circle (at 16 2.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 14b thru_hole circle (at 15 4.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 13b thru_hole circle (at 14 2.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 12b thru_hole circle (at 13 4.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 11b thru_hole circle (at 10 2.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 10b thru_hole circle (at 9 4.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 9b thru_hole circle (at 8 2.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 8b thru_hole circle (at 7 4.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 7b thru_hole circle (at 6 2.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 6b thru_hole circle (at 5 4.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 5b thru_hole circle (at 4 2.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 4b thru_hole circle (at 3 4.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 3b thru_hole circle (at 2 2.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 2b thru_hole circle (at 1 4.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 1b thru_hole circle (at 0 2.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 18a thru_hole circle (at 19 -2) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 17a thru_hole circle (at 18 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 16a thru_hole circle (at 17 -2) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 15a thru_hole circle (at 16 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 14a thru_hole circle (at 15 -2) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 13a thru_hole circle (at 14 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 12a thru_hole circle (at 13 -2) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 11a thru_hole circle (at 10 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 10a thru_hole circle (at 9 -2) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 9a thru_hole circle (at 8 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 8a thru_hole circle (at 7 -2) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 7a thru_hole circle (at 6 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 6a thru_hole circle (at 5 -2) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 5a thru_hole circle (at 4 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 4a thru_hole circle (at 3 -2) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 3a thru_hole circle (at 2 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 2a thru_hole circle (at 1 -2) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 1a thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
)
